**TDS in parts per million (PPM)**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 0 | 50 | 100 | 200 | 300 | 400 | 500 |
|  |  |  |  |  |  |  |

U.S.A. EPA’s

Maximum

Containment level

Marginally Acceptable

Reverse Osmosis, deionization, microfiltration, distillation, etc.

High TDS water from the tap or mineral springs

Carbon filtration, mountain

springs or aquifers

Average Tap Water